#### Lecture Series Online (2020) Hydro-Geography MSC 4th + BS 8th Lecture#3. Date: 17-03-2020

**Flood Benefits, Safety Planning, Flood Control, Forecasting and World Deadliest Flood**

1. **Benefits**

Floods (in particular more frequent or smaller floods) can also bring many benefits, such as recharging [ground water](https://en.wikipedia.org/wiki/Ground_water), making soil more [fertile](https://en.wikipedia.org/wiki/Fertility_%28soil%29) and increasing [nutrients](https://en.wikipedia.org/wiki/Nutrient) in some soils. Flood waters provide much needed water resources in [arid](https://en.wikipedia.org/wiki/Arid) and [semi-arid](https://en.wikipedia.org/wiki/Semi-arid) regions where precipitation can be very unevenly distributed throughout the year and kills pests in the farming land. Freshwater floods particularly play an important role in maintaining [ecosystems](https://en.wikipedia.org/wiki/Ecosystem) in river corridors and are a key factor in maintaining floodplain [biodiversity](https://en.wikipedia.org/wiki/Biodiversity). Flooding can spread nutrients to lakes and rivers, which can lead to increased [biomass](https://en.wikipedia.org/wiki/Biomass) and improved [fisheries](https://en.wikipedia.org/wiki/Fisheries) for a few years.

For some fish species, an inundated floodplain may form a highly suitable location for [spawning](https://en.wikipedia.org/wiki/Spawning) with few predators and enhanced levels of nutrients or food. Fish, such as the [weather fish](https://en.wikipedia.org/wiki/Weather_fish), make use of floods in order to reach new habitats. Bird populations may also profit from the boost in food production caused by flooding.

Periodic flooding was essential to the well-being of ancient communities along the [Tigris-Euphrates](https://en.wikipedia.org/wiki/Tigris-Euphrates) Rivers, the [Nile River](https://en.wikipedia.org/wiki/Nile_River), the [Indus River](https://en.wikipedia.org/wiki/Indus_River), the [Ganges](https://en.wikipedia.org/wiki/Ganges) and the [Yellow River](https://en.wikipedia.org/wiki/Yellow_River) among others. The viability of [hydropower](https://en.wikipedia.org/wiki/Hydropower), a renewable source of energy, is also higher in flood prone regions.

1. **Flood Safety Planning**

In the United States, the [National Weather Service](https://en.wikipedia.org/wiki/National_Weather_Service) gives out the advice Turn Around, Don't Drown" for floods; that is, it recommends that people get out of the area of a flood, rather than trying to cross it. At the most basic level, the best defense against floods is to seek higher ground for high-value uses while balancing the foreseeable risks with the benefits of occupying flood hazard zones. Critical community-safety facilities, such as hospitals, emergency-operations centers, and police, fire, and [rescue](https://en.wikipedia.org/wiki/Rescue) services, should be built in areas least at risk of flooding. Structures, such as bridges, that must unavoidably be in flood hazard areas should be designed to withstand flooding. Areas most at risk for flooding could be put to valuable uses that could be abandoned temporarily as people retreat to safer areas when a flood is imminent.

Planning for flood safety involves many aspects of analysis and engineering, including:

* observation of previous and present flood heights and inundated areas,
* statistical, [hydrologic](https://en.wikipedia.org/wiki/Hydrologic), and hydraulic model analyses,
* mapping inundated areas and flood heights for future flood scenarios,
* long-term [land use planning](https://en.wikipedia.org/wiki/Land_use_planning) and regulation,
* [engineering design](https://en.wikipedia.org/wiki/Engineering_design) and construction of structures to control or withstand flooding,
* intermediate-term monitoring, [forecasting](https://en.wikipedia.org/wiki/Flood_forecasting), and emergency-response planning, and
* Short term monitoring, [warning](https://en.wikipedia.org/wiki/Flood_warning), and response operations.

Each topic presents distinct yet related questions with varying scope and scale in time, space, and the people involved. Attempts to understand and manage the mechanisms at work in floodplains have been made for at least six millennia.

In the United States, the Association of State Flood plain Managers works to promote education, policies, and activities that mitigate current and future losses, costs, and human suffering caused by flooding and to protect the natural and beneficial functions of floodplains – all without causing adverse impacts. A portfolio of [best practice](https://en.wikipedia.org/wiki/Best_practice) examples for [disaster mitigation](https://en.wikipedia.org/wiki/Disaster_mitigation) in the United States is available from the Federal Emergency Management Agency.

1. **Flood Control**

In many countries around the world, waterways prone to floods are often carefully managed. Defenses such as [detention basins](https://en.wikipedia.org/wiki/Detention_basin), [levees](https://en.wikipedia.org/wiki/Levee), [bunds](https://en.wikipedia.org/wiki/Bunding), [reservoirs](https://en.wikipedia.org/wiki/Reservoir_%28water%29), and [weirs](https://en.wikipedia.org/wiki/Weir) are used to prevent waterways from overflowing their banks. When these defenses fail, emergency measures such as [sandbags](https://en.wikipedia.org/wiki/Sandbag) or portable inflatable tubes are often used to try to stem flooding. Coastal flooding has been addressed in portions of Europe and the Americas with [coastal defenses](https://en.wikipedia.org/wiki/Coastal_management), such as [sea walls](https://en.wikipedia.org/wiki/Sea_wall), [beach nourishment](https://en.wikipedia.org/wiki/Beach_nourishment), and [barrier islands](https://en.wikipedia.org/wiki/Barrier_island).

In the riparian zone near rivers and streams, [erosion control](https://en.wikipedia.org/wiki/Erosion_control) measures can be taken to try to slow down or reverse the natural forces that cause many waterways to meander over long periods of time. Flood controls, such as dams, can be built and maintained over time to try to reduce the occurrence and severity of floods as well. In the United States, the [U.S. Army Corps of Engineers](https://en.wikipedia.org/wiki/U.S._Army_Corps_of_Engineers) maintains a network of such flood control dams.

In areas prone to urban flooding, one solution is the repair and expansion of man-made sewer systems and storm water infrastructure. Another strategy is to reduce impervious surfaces in streets, parking lots and buildings through natural drainage channels, [porous paving](https://en.wikipedia.org/wiki/Porous_paving), and [wetlands](https://en.wikipedia.org/wiki/Wetlands) (collectively known as [green infrastructure](https://en.wikipedia.org/wiki/Green_infrastructure) or [sustainable urban drainage systems](https://en.wikipedia.org/wiki/Sustainable_urban_drainage_systems) (SUDS)). Areas identified as flood-prone can be converted into parks and playgrounds that can tolerate occasional flooding. Ordinances can be adopted to require developers to retain storm water on site and require buildings to be elevated, protected by [floodwalls](https://en.wikipedia.org/wiki/Floodwall) and [levees](https://en.wikipedia.org/wiki/Levees), or designed to withstand temporary inundation. Property owners can also invest in solutions themselves, such as re-landscaping their property to take the flow of water away from their building and installing [rain barrels](https://en.wikipedia.org/wiki/Rain_barrels), [sump pumps](https://en.wikipedia.org/wiki/Sump_pump), and [check valves](https://en.wikipedia.org/wiki/Check_valve).

1. **Flood forecasting and**[**flood warning**](https://en.wikipedia.org/wiki/Flood_warning)

Anticipating floods before they occur allows for precautions to be taken and people to be warned so that they can be prepared in advance for flooding conditions. For example, farmers can remove animals from low-lying areas and utility services can put in place emergency provisions to re-route services if needed. Emergency services can also make provisions to have enough resources available ahead of time to respond to emergencies as they occur. People can evacuate areas to be flooded.

In order to make the most accurate flood forecasts for [waterways](https://en.wikipedia.org/wiki/Waterway), it is best to have a long time-series of historical data that relates [stream flows](https://en.wikipedia.org/wiki/Stream_flow) to measure past rainfall events. Coupling this historical information with [real-time knowledge](https://en.wikipedia.org/wiki/Real-time_data) about volumetric capacity in catchment areas, such as spare capacity in reservoirs, ground-water levels, and the degree of [saturation](https://en.wikipedia.org/wiki/Phreatic_zone) of area [aquifers](https://en.wikipedia.org/wiki/Aquifer) is also needed in order to make the most accurate flood forecasts.

[Radar](https://en.wikipedia.org/wiki/Weather_radar) estimates of rainfall and general [weather forecasting](https://en.wikipedia.org/wiki/Weather_forecasting) techniques are also important components of good flood forecasting. In areas where good quality data is available, the intensity and height of a flood can be predicted with fairly good accuracy and plenty of lead time. The output of a flood forecast is typically a maximum expected water level and the likely time of its arrival at key locations along a waterway, and it also may allow for the computation of the likely statistical return period of a flood. In many developed countries, urban areas at risk of flooding are protected against a 100-year flood – that is a flood that has a probability of around 63% of occurring in any 100-year period of time.

In the United States, an integrated approach to real-time hydrologic computer modeling utilizes observed data from the [U.S. Geological Survey](https://en.wikipedia.org/wiki/U.S._Geological_Survey) (USGS), various [cooperative observing networks](https://en.wikipedia.org/wiki/Weather_spotting), various [automated weather sensors](https://en.wikipedia.org/wiki/Automated_airport_weather_station), the [NOAA](https://en.wikipedia.org/wiki/NOAA) National Operational Hydrologic Remote Sensing Center (NOHRSC), various [hydroelectric](https://en.wikipedia.org/wiki/Hydroelectric) companies, etc. combined with [quantitative precipitation forecasts](https://en.wikipedia.org/wiki/Quantitative_precipitation_forecast) (QPF) of expected rainfall and/or snow melt to generate daily or as-needed hydrologic forecasts.[[34]](https://en.wikipedia.org/wiki/Flood#cite_note-Advanced_Hydrologic_Prediction_System-34) The NWS also cooperates with [Environment Canada](https://en.wikipedia.org/wiki/Environment_Canada) on hydrologic forecasts that affect both the US and Canada, like in the area of the [Saint Lawrence Seaway](https://en.wikipedia.org/wiki/Saint_Lawrence_Seaway).

The Global Flood Monitoring System, "GFMS," a computer tool which maps flood conditions worldwide, is available [online](http://flood.umd.edu/). Users anywhere in the world can use GFMS to determine when floods may occur in their area. GFMS uses precipitation data from [NASA](https://en.wikipedia.org/wiki/NASA)'s Earth observing satellites and the [Global Precipitation Measurement satellite](https://en.wikipedia.org/w/index.php?title=Global_Precipitation_Measurement_satellite&action=edit&redlink=1), "GPM." Rainfall data from GPM is combined with a land surface model that incorporates vegetation cover, soil type, and terrain to determine how much water is soaking into the ground, and how much water is flowing into stream flow.

Users can view statistics for rainfall, stream flow, water depth, and flooding every 3 hours, at each 12 [kilometer](https://en.wikipedia.org/wiki/Kilometer) grid point on a global map. Forecasts for these parameters are 5 days into the future. Users can zoom in to see inundation maps (areas estimated to be covered with water) in 1 kilometer resolution. Deadliest floods.

1. ***List of deadliest floods***

Below is a list of the deadliest floods worldwide, showing events with death tolls at or above 100,000 individuals

| **Death toll** | **Event** | **Location** | **Date** |
| --- | --- | --- | --- |
| 2,500,000–3,700,000[[41]](https://en.wikipedia.org/wiki/Flood#cite_note-41) | [1931 China floods](https://en.wikipedia.org/wiki/1931_China_floods) | [China](https://en.wikipedia.org/wiki/China) | 1931 |
| 900,000–2,000,000 | [1887 Yellow River flood](https://en.wikipedia.org/wiki/1887_Yellow_River_flood) | [China](https://en.wikipedia.org/wiki/China) | 1887 |
| 500,000–700,000 | [1938 Yellow River flood](https://en.wikipedia.org/wiki/1938_Yellow_River_flood) | China | 1938 |
| 231,000 | [Banqiao Dam](https://en.wikipedia.org/wiki/Banqiao_Dam) failure, result of [Typhoon Nina](https://en.wikipedia.org/wiki/Typhoon_Nina_%281975%29). Approximately 86,000 people died from flooding and another 145,000 died during subsequent disease. | China | 1975 |
| 230,000 | [2004 Indian Ocean tsunami](https://en.wikipedia.org/wiki/2004_Indian_Ocean_earthquake) | [Indonesia](https://en.wikipedia.org/wiki/Indonesia) | 2004 |
| 145,000 | 1935 [Yangtze](https://en.wikipedia.org/wiki/Yangtze) river flood | China | 1935 |
| 100,000 | [Hanoi](https://en.wikipedia.org/wiki/Hanoi) and [Red River Delta](https://en.wikipedia.org/wiki/Red_River_Delta) flood | [North Vietnam](https://en.wikipedia.org/wiki/North_Vietnam) | 1971 |
| 100,000 | 1911 [Yangtze](https://en.wikipedia.org/wiki/Yangtze) river flood | China | 1911 |

***Thank You***